<   COMPANY LETTER HEAD   >

LETTER OF INDEMNITY FOR VEHICLES IN CARGO TRANSPORT UNITS
TO: 
DANGEROUS GOODS MANAGER, 
PORT KLANG AUTHORITY
MAIL BAG SERVICE 202, JALAN PELABUHAN UTARA 
42005 PORT KLANG, SELANGOR, MALAYSIA

	VESSEL NAME
	

	SHIP CALL NUMBER
	

	ETA			
	

	PORT OPERATOR
(*to select either one)
	NORTHPORT
	
	WESTPORTS
	

	CONTAINER(s) NUMBER
	

	VEHICLE MODEL
	

	VEHICLE QUANTITY
	

	PORT OF LOADING
	

	PORT OF DISCHARGE
	

	SHIPPER
	

	CONSIGNEE
	

	ENGINE VARIANT (*to select)
	Petrol
	
	Diesel
	
	Gas
	
	Hybrid/HEV/PHEV
	
	EV
	

	BATTERY TYPE
(*Only applicable for Hybrid and EV)
	Wet / Dry
	
	Metallic Sodium
	
	Sodium Alloy
	

	
	Lithium Ion
	
	Lithium Metal
	
	Sodium Ion
	



Notes: Vehicles that do not comply with SP961 must be classified as Class 9 and transported in accordance with the requirements specified in SP962.

We hereby confirm that this shipment meets the requirements of Special Provision 961 of IMDG Code 42-24 in all aspects.

We, the undersigned, do hereby undertake to hold you free and harmless from any claim that may arise in connection with the above-mentioned certificate.



    ________________________________________
  (Signature of declarant with company rubber stamp)

Name	: 
Position	: 
Date		:

Only applicable for;
	UN NUMBER
	PROPER SHIPPING NAME

	3166
	VEHICLE, FLAMMABLE GAS POWERED or VEHICLE, FLAMMABLE LIQUID POWERED or VEHICLE, FUEL CELL, FLAMMABLE GAS POWERED or VEHICLE, FUEL CELL, FLAMMABLE LIQUID POWERED

	3171
	BATTERY-POWERED VEHICLE

	3556
	VEHICLE, LITHIUM ION BATTERY POWERED

	3557
	VEHICLE, LITHIUM METAL BATTERY POWERED

	3558
	VEHICLE, SODIUM ION BATTERY POWERED



Special provision 961

Vehicles are not subject to the provisions of this Code other than those in P912, SP388, and SP977 when applicable, if any of the following conditions are met:
.1 vehicles are stowed on the vehicle, special category and ro-ro spaces or on the weather deck of a ro-ro ship or a cargo space designated by the Administration (flag State) in accordance with SOLAS 74, chapter II-2, regulation 20 as specifically designed and approved for the carriage of vehicles, and there are no signs of leakage from the battery, engine, fuel cell, compressed gas cylinder or accumulator, or fuel tank when applicable. When packed in a cargo transport unit the exception does not apply to container cargo spaces of a ro-ro ship.
.2 vehicles powered by a flammable liquid fuel with a flashpoint of 38°C or above, there are no leaks in any portion of the fuel system, the fuel tank(s) contains 450 L of fuel or less and installed batteries are protected from short-circuit;
.3	vehicles powered by a flammable liquid fuel with a flashpoint less than 38°C, the fuel tank(s) are empty and installed batteries are protected from short circuit. Vehicles are considered to be empty of flammable liquid fuel when the fuel tank has been drained and the vehicles cannot be operated due to a lack of fuel. Engine components such as fuel lines, fuel filters and injectors do not need to be cleaned, drained or purged to be considered empty. The fuel tank does not need to be cleaned or purged;
.4	vehicles powered by a flammable gas (liquefied or compressed), the fuel tank(s) are empty and the positive pressure in the tank does not exceed 2 bar, the fuel shut-off or isolation valve is closed and secured, and installed batteries are protected from short circuit;
.5	vehicles solely powered by a wet or dry electric storage battery or a sodium battery, and the battery is protected from short circuit.
.6	vehicles solely powered by a sodium ion battery, and the battery is short-circuited in a way that the battery does not contain electrical energy. The short circuiting shall be easily identifiable (e.g. busbar between terminals).



Special provision 962

Vehicles, not meeting the conditions of special provision 961 shall be assigned to class 9 and shall meet the following requirements:

.1 	vehicles shall not show signs of leakage from batteries, engines, fuel cells, compressed gas cylinders or accumulators, or fuel tank(s) when applicable;

.2 	for flammable liquid powered vehicles the fuel tank(s) containing the flammable liquid shall not be more than one fourth full, and in any case the flammable liquid shall not exceed 250 L unless otherwise approved by the competent authority;

.3 	for flammable gas powered vehicles, the fuel shut-off valve of the fuel tank(s) shall be securely closed;

.4 	installed batteries shall meet the provisions of SP388 or SP977, as applicable, and be protected from damage, short circuit, and accidental activation during transport.

The provisions of this Code relevant to marking, labelling, placarding and marine pollutants shall only apply to vehicles that are fully enclosed by packagings, crates or other means that prevent ready identification (e.g., overpack).
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